**Electric Utility Vehicle- Verification of Competency (VoC)**

|  |  |
| --- | --- |
| Requirement | COMPLETE(initials) |
| does the worker hold a current c class drivers license not currently under suspension |  |
| Location of keys and any reservation system for booking the EUV |  |
| Safely entering and exiting the golf cart |  |
| operation of seatbelts |  |
| operation of brakes, indicators, lights, reversing alert, and gears |  |
| Reversing and parking demonstration |  |
| Inductee practices driving, including reversing and parking, under supervision of an approved operator delegated  |  |
| operating on campus roads, including speed limits and cornering |  |
| operating on paths with pedestrians present |  |
| navigating speed humps and other traffic slowing infrastructure on campus roads |  |
| loading and unloading the golf cart  |  |
| procedure for charging the golf cart |  |
| procedure for moving golf cart into and out of assigned storage locations |  |
| golf cart must not to exceed 30km/h at any time |  |
| maximum speed on pathways and within the pedestrian precint must not exceed walking pace or 5km/hr |  |
| Instruction given for operation in different weather conditions |  |
| operators must stop at all ‘blind’ intersections, sound the horn then proceed with caution |  |

\*Area Managers must store copies of the completed VOC for workers in their areas\*